> | # UMDsend ## Description This component is a demonstrator for component writing. It is intended to send text to an infodriver slot, where that slot is then sent to a UMD by a BNCS automatic. The user should set the Infodriver ID and Slot number as part of the Visual Design edit. ## Commands
> Name | Type | Use
> --- | --- | ---
> text | String | Text to send to the UMD
> InfoDriverID | Number | Infodriver ID that drives UMD
> Slot | Number | Slot number for this UMD
> ## Notifications
> Name | Use
> --- | ---
> None |
> ## Stylesheets
> Name | Use
> --- | ---
> None |
## Developers Notes The script host component shuld be set to 160 pixels wide by 30 lines high.
Copyright BBC 2016