Driver name:  SonyViscaV3NoSSE.EXE

Function: Control Visca Protocol Cameras

There are three versions of the driver: 
  a)	SonyViscaV3dot0.exe
  b)	SonyViscaV3dot1.exe
  c)	SonyViscaV3NoSSE.exe

Version c is a special for use on Intel Atom computers that do not support
the SSE instruction set. One such unit is a small FIT pc used to control
two cameras in Bredon Wing.

See the SonyViscaV3dot0.PDF document for information on slot use.

Andy Woodhouse
30th May 2017